(footprint "MDKM24"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -23 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "MDKM24"
		(at 0 -21.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_line
		(start -15.875 -14.099)
		(end -15.875 14.099)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -12.525 -15.099)
		(end -14.875 -15.099)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -11.944 -15.75)
		(end -11.944 -15.68)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.905 15.099)
		(end -14.875 15.099)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -4.324 15.75)
		(end -4.324 15.68)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 3.324 -16.75)
		(end -10.944 -16.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.324 -15.68)
		(end 4.324 -15.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 4.905 -15.099)
		(end 14.875 -15.099)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 10.944 16.75)
		(end -3.324 16.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 11.944 15.68)
		(end 11.944 15.75)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 14.875 15.099)
		(end 12.525 15.099)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 15.875 -14.099)
		(end 15.875 14.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -15.875 -14.099)
		(mid -15.582107 -14.806107)
		(end -14.875 -15.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -14.875 15.099)
		(mid -15.582107 14.806107)
		(end -15.875 14.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -11.944 -15.75)
		(mid -11.651107 -16.457107)
		(end -10.944 -16.75)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -11.944 -15.68)
		(mid -12.114171 -15.269171)
		(end -12.525 -15.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -4.905 15.099)
		(mid -4.494171 15.269171)
		(end -4.324 15.68)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start -3.324 16.75)
		(mid -4.031107 16.457107)
		(end -4.324 15.75)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 3.324 -16.75)
		(mid 4.031107 -16.457107)
		(end 4.324 -15.75)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 4.905 -15.099)
		(mid 4.494171 -15.269171)
		(end 4.324 -15.68)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 11.944 15.68)
		(mid 12.114171 15.269171)
		(end 12.525 15.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 11.944 15.75)
		(mid 11.651107 16.457107)
		(end 10.944 16.75)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 14.875 -15.099)
		(mid 15.582107 -14.806107)
		(end 15.875 -14.099)
		(layer "Edge.Cuts")
	)
	(fp_arc
		(start 15.875 14.099)
		(mid 15.582107 14.806107)
		(end 14.875 15.099)
		(layer "Edge.Cuts")
	)
	(fp_text user "${REFERENCE}"
		(at 0 -20 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -13.225 -17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at 5.605 -17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at 8.145 -17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at 10.685 -17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 13.225 -17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at -13.225 17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at -10.685 17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at -8.145 17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "9" smd roundrect
		(at -5.605 17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(pad "10" smd roundrect
		(at 13.225 17.015)
		(size 1.8 3.07)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.1111111111)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
)
